
* In the networks Below, assume all routers run RIP and all link costs are 1. Show the initial state tables and the routing tables after convergence.

.



If the link to Network 205.5.5.0 failed and R4 set the cost to infinity , what will be happen into the folowing situations:

* R1 send updates first to R4.
* R4 send the updates to R1.