**King Saud University**

**College Of Computer & Information Sciences**

**Department Of Computer Sciences**

**Tutorial 1 Fall 15**

**(Computer Networks CSC 329)**

1. Define the concept of layer and protocol.
2. Explain the concepts of

* Physical medium link
* Network node ( router , switch , hub)

1. Explain the concepts of connection oriented and connectionless communication.
2. **OSI Model and its layers**
3. **Define router**

Small physical devices that joins multiple n/w together

Eg. Layer 3 gateway devices.

1. **Network names by Scale :**

**PAN ( personal area network , using Blue tooth ) < LAN ( for building , using wifi or ethernet) < MAN < WAN < INTERNET**

1. **Example of Networks:**

Wifi,, Mobile phone , blue tooth, telephone, satellite etc..

1. Explain the concept of communication latency between two communication entities through network.
2. Explain the concepts of :

* Packet transmission time ( sending time ).
* Packet transition delay ( in nodes ).
* Propagation delay.

1. Between A and B, the communication has these characteristics

500 m

B

A

Packet length - 1500 bytes

Channel speed - 10 Mbits/sec

Propagation delay - 5 msec/km ≡ 200.103 km/s

Given these parameters, calculate the:

* Packet transmission time
* **Propagation delay**

Time taken by from one end to other end of network.

S……………………R

First bit is travelled but last bit is still at sender point

Propogation delay depends on the distance and velocity.

Tp = d / v

In case of Optical fiber : v = 3 \* 10 8  \* 0.7

= 2.1 \* 10 8 m/s

**Eg.**

**Distance = 21 km, v = 2.1 \* 10 8 m/s find Tp in sec, millisecond and Microsecond**

**Tp =( 2.1 \* 10 3 )/( 2.1 \* 10 8 ) = 10 -5  sec**

**= 10 -2  millisecond**

**= 10 Microsecond**

1. **Transmission delay :**

Time taken to transmit from a host to put the data packet on out going link.

Transmission delay = length of the packet / bandwidth = L / B

1. **. Bandwidth = 1 bps and Data = 10 bits find Transmission delay :**

Transmission delay = L / B = 10 / 1 = 10 sec

1. **. L = 1000 bits, BW = 1 kbps find Transmission time :**

Tt = L / B = 1000/ 1000 = 1 sec.

1. **L = 1 Kb, Bandwidth = 1 kbps find Tt :**

1 Kb = 1024 b

1 kbps = 1000 bps

Tt = L / B = 1024 b/ 1000 bps = 1.024

**Queuing Delay :**

Amount of time packet being seated in buffer before being processed.

Depends on the processing delay