**QUIZ # 3**

**Section 32690**

**Aggregates**

Take **5 minutes** to answer the following questions

**Q1** The Sand Equivalent (SE) value for two materials A and B is as follows:

SEA = 70% and SEB = 35%.

2-1 which of the two materials contains more fines? And why do we care for fines in asphalt concrete mix?[5 marks]

**Q2** Briefly state the difference between the bulk specific gravity and the apparent specific gravity [5 marks].