**Windows-Based Port Connection Status**

In this lab you will use the Windows netstat command to analyze an FTP connection and an HTTP connection to a server.

***Materials and Setup***

You will need the following:

* Windows 7
* Windows 2008 Server

***Lab Steps at a Glance***

1. Log on to the Windows 7and Windows 2008 Server PCs.
2. Use the netstat command to look at the open ports on the Windows 2008 Server machine.
3. From the Windows 7 machine, establish an FTP connection and an HTTP connection to the Windows 2008 Server machine.
4. Use the netstat command to look at the connections on the Windows 2008 Server machine.
5. Log off from both the Windows 2008 Server and Windows 7 PCs